Ductile damage **model calibration for structural stainless steel using ABAQUS software: An overview.**

*Please note: This is not the final representation of the manuscript.*

Authors: Bommin Bam, Suman Kumar Mushahary.

Abstract

A practical method for calibration of the phenomenological damage model for stainless steel grades IRS 350 CR (equivalent grade- ASTM A709 50 CR or ASTM A1010) and IRS 450 CR (equivalent grade- not defined) using the full-range engineering stress-strain curves from tensile coupon test.